Items for set-up:

**Consumables/ spare parts:**

|  |  |
| --- | --- |
| **ITEM DESCRIPTION** | **UNIT OF MEASURE** |
| TEMPERATURE LIMITER IDENTITY #:7824 | PCS |
| RUBBER-SCRAPPER  -type 4x9”  -borehole distance 63.5mm  -strong version 35mm  -with 3 dredges | Pcs |
| BEARING HOUSING FLANGED 516 B IDENTITY#:9092 | PCS |
| BEARING HOUSING FLANGED 516 A IDENTITY#:9095 | PCS |
| FOLDABLE LIFTING BOLTS IDENTITY#:513  -made of stainless steel for drivers | PCS |
| SELF-LOCKING HEXAGON NUTS, A2 IDENTITY#:287 | PCS |
| BUSH FOR CHAIN T=80 IDENTITY #:567 | PCS |
| SHIFT BOLT M 10 IDENTITY#:5353 | PCS |
| BOLZ FOR CLIP CHAIN IDENTITY#:5352 | PCS |
| TAPPETS IDENTITY#:1302 | PCS |
| TAPPETS IDENTITY#:3227 | PCS |
| EMERGENCY STOP SWITCH IDENTITY#:10627 | PCS |
| CHAIN WHEEL DISC D=617mm IDENTITY#:10375 | PCS |
| STUB AXLE IDENTITY#:2774  -for deflection station plug-in chain 4”  -square 60mm  -with wheel bolts M18x1.5  -with spherical collar nut A18 DIN 74361 | PCS |
| SPRING BALANCER 60-70 KG IDENTITY#:9290  -rope pull out 3m | PCS |
| KUGELLAGER FŪR BUSTER VI JARVIS-ART. 1921385  Identity#:7725 | PCS |
| KUGELLAGER FŪR BUSTER VI JARVIS-ART. 1921386  Identity#:7726 | PCS |
| CROSS SWITCH 2” IDENTITY#:8551  -mounted on the plate  -consoles to be turned depending on incoming hook side  -mounting pin diam. 49.5mm  -top edge tuberail – top edge mounting plate  150mm  -with safety of tube endings + operating lever  -steel parts hot galvanized  -screw and pins stainless steel | PCS |
| CHAIN WHEEL DISC D=760 mm IDENTITY#:11942 | PCS |
| KLINGE FŪR HOHLSTECHMESSER IDENTITY#:8241 | PCS |
| COMPACT THERMOMETER IDENTITY#:11351 | PCS |
| DIAPHRAGM (EH1973) | PCS |
| BEARING #6010 rubber seal type | PCS |
| BEARING #6208 rubber seal type | PCS |
| BEARING #6207 rubber seal type | PCS |
|  |  |