**SUPPLY OF APOLLO CONVENTIONAL CONTROL PANEL& DEVICES**

**-1 unit SIGMA CP**-4 zone conventional fire alarm control panel 4x Monitored detection zones compatible with many conventional detection devices, 2x Monitored sounder outputs-500mA per output, VFCO barriers, Integral 3 amp PSU, Space for 2 x 12V 7AH SLA batteries M2 Surface amount enclosure 385mm(W) x 310mm(H) x 50mm(D) (Made in UK) (2years warranty), Model: K11040 M2

**-2 pcs Back up battery** ( 1 year warranty) Model: 12V 7.2AH YUASA

**-9 pcs D-128 Resettable call point ( Red)** Made in Malaysia ( 1year warranty) model: d-128

**-9 pcs DEMCO Sounder and Strobe Light Combined** (1year warranty) Model: D-115/154L

**-9 pcs Series 65 Optical Smoke Detector with flashing LED with 45681-200APO Series 65 Standard Base** ( 5years warranty) Model: 55000-316APO+45681+200APO

**-2 pcs Series 65 Optical Heat Detector with flashing LED with series 65 Standard base** ( 5 years warranty) Model: 55000-316APO+45681-200APO

**-3 rolls TF WIRE 1.25mm #16 2 core** (Thermoplastic Fixture) Model: PHILPLEX

**-1 pc Surge Protection**, Model: Surge Protector

**-1 pc 1000VA 230V AVR Universal Sockets** Model: UPS 1KVA

**UNIT of MEASURE: LOT**