RICEMILL 2

1.MULTIMEDIA DEPTH SEDIMENT FILTER 60GPM = UNIT

>TOP MOUNTED

>FRP TANK 36 X 72 WAVE CYBER BEIGE

>RUNXIN HEAD F77B1 SEDIMENT TIMER TYPE 4"

>with pebbles, quarts sand, silica sand, anthracite, pipe gray 1 1/2

2. ACTIVATED CARBON FILTER 60GPM = UNIT

>TOP MOUNTED

>FRP TANK 36 X 72 WAVE CYBER BIEGE

>RUNXIN HEAD F77B1 SEDIMENT TIMER TYPE 4"

>with pebbles , pure prime activated carbon 8 x 12, pipe gray 1 1/2

3. WATER SOFTENER 80GPM = UNIT

>TOP MOUNTED

>RUNXIN DIGITAL HEAD F95A3 SOFT (120m3/h) METER

>FRP TANK 48 X 72 WAVE CYBER BEIGE

>BRINE TANK 290L (WHITE)

>with pebbles, high grade resin H-C 100E, pipe gray 1 1/2

4. WATER SOFTENER 15GPM = UNIT

>TOP MOUNTED

>FRP TANK 24 X 72 WAVE CYBER BEIGE

>RUNXIN DIGITAL HEAD F99A3 SOFTENER (15m3/h) METER

>BRINE TANK 180L (WHITE)

>with pebbles, high grade resin H-C 100E, pipe gray 1 1/2