RICEMILL 2

1.AWNING WINDOW HP-85 GLASS 6mm CLEAR TEMPERED

>1500mm (W) x 300mm (H)

>1.44mm Aluminum Profile Thickness; Powder coated

>Sand Gray Finish; German Technology Mechanism

>with Security Hard mesh Screen

>Outside/Inside color: Sand Gray

>Screen: Gray

2.CASEMENT WINDOW HP-85 GLASS 6mm CLEAR TEMPERED

>1800mm (W) x 1200 (H)

>1.44mm Aluminum Profile Thickness; Powder coated

>Sand Gray Finish; German Technology Mechanism

>with Security Hard Mesh Screen

>Outside/Inside color: Sand Gray

>Screen: Gray

3. CASEMENT WINDOW HP-85 GLASS 6mm CLEAR TEMPERED

>1000mm (W) x 600mm (H)

>1.44mm Aluminum Profile Thickness; Powder coated

>Sand Gray Finish; German Technology Mechanism

>with Security Hard Mesh Screen

>Outside/Inside color: Sand Gray

>Screen: Gray

4.SLIDING DOOR HP-134 GLASS 6mm CLEAR TEMPERED

>1700mm (W) x 2100mm (H)

>2.0mm Aluminum Profile Thickness; Powder coated

>Sand Gray Finish; German Technology Mechanism

>Using Flat Track

>Outside/Inside color: Sand Gray

>Screen: Gray

5.SHOWER ENCLOSURE HP-FRAMELESS GLASS 6mm CLEAR TEMPERED

>825mm (W) x 2100mm (H)

>Glass Partition Using Stainless Shower clip

>Outside/Inside color: Gray